# Marged Parts
Due to request, the housing, front cover, electronics box and electronics cover has been merged. It is huge and can only be printed on larger printers with an excruciating long print time.

# Print Settings for 3D printed Parts
Slicing has been done in PrusaSlicer but can be sliced in preferred slicing software. The settings below can be changed at the expense of the user. Recommended Materials are that of PETG and ASA.

## PrusaSlicer Settings

*   Layer Height: 0.3mm
*   Extrusion Width: 0.4mm
*   Infill Percentage: 40%
*   Infill Type: Gyroid
*   Wall Count: 5
*   Solid Top/Bottom Layers: 4